# Test case for basic movement on polar printers
CONFIG ../../config/example-polar.cfg
DICTIONARY atmega2560-16mhz.dict

; Start by homing the printer.
G28
G90
G1 F6000

; Z / X / Y moves
G1 Z1
G1 X1
G1 Y1

; Delayed moves
G1 Y2
G4 P100
G1 Y1.5
M400
G1 Y1

; diagonal moves
G1 X10 Y0
G1 X1 Z2
G1 X0 Y1 Z1

; extrude only moves
G1 E1
G1 E0

; regular extrude move
G1 X10 Y0 E.01
